Proposal for amendments to amend UN Regulation No. 157

The text below is based on GRVA-10-25 and includes modifications introduced during the tenth session of the Working Party on Automated/Autonomous and Connected vehicles (GRVA)

Modifications to the existing text of UN Regulation No. 157 are marked in **bold** for new or ~~strikethrough~~ for deleted characters.

Proposal:

*Paragraph 2.5.*, amend to read:

“2.5. "*Unplanned event*" is a situation which is unknown in advance, but assumed as very likely in happening~~, e.g. road construction, inclement weather, approaching emergency vehicle, missing lane marking, load falling from truck (collision)~~ and which requires a transition demand. **This may include: road construction, inclement weather, approaching emergency vehicles/enforcement vehicles, missing lane markings, load falling from truck.**”

*Paragraph 5.1.2.,* amend to read:

“5.1.2. The activated system shall comply with traffic rules relating to the DDT in the country of operation**, including responding to emergency/enforcement vehicles**.”