|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.15/AC.2/2021/19 | |
| United Nations logo | **Economic and Social Council** | | Distr.: General  21 May 2021  English  Original: French |

**Economic Commission for Europe**

Inland Transport Committee

**Joint Meeting of Experts on the Regulations annexed to the   
European Agreement concerning the International Carriage  
of Dangerous Goods by Inland Waterways (ADN)   
(ADN Safety Committee)**

**Thirty-eighth session**

Geneva, 23–27 August 2021

Item 4 (b) of the provisional agenda

**Proposals for amendments to the Regulations annexed to ADN: Other proposals**

Various amendments and corrections to ADN 2021 subject to notification

Transmitted by the Government of Germany[[1]](#footnote-1)\*, [[2]](#footnote-2)\*\*

1. Germany proposes that the Safety Committee make the following amendments and corrections to the Regulations annexed to ADN (ADN 2021).

Table A

2. Amendments in all language versions:

| *UN No.* | *Order number* | *Name and description* | *Packing group* | *Amendment* | *Justification* |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
| 2381 | 1 | DIMETHYL DISULFIDE | II | Add special provision 802 in column (6) of Table A. | In ADR/RID, column (18) of Table A shows the corresponding special provision CV28/CW28 |
| 3440 | 1 | SELENIUM COMPOUND, LIQUID, N.O.S. | I | Add special provisi on 563 in column (6) of Table A. | As in Table A of ADR/RID |
| 3440 | 2 | SELENIUM COMPOUND, LIQUID, N.O.S. | II |
| 3440 | 3 | SELENIUM COMPOUND, LIQUID, N.O.S. | III |
| 3483 | 1 | MOTOR FUEL ANTI-KNOCK MIXTURE, FLAMMABLE |  | Add special provision 802 in column (6) of Table A. | In ADR/RID, column (18) of Table A shows the corresponding special provision CV28/CW28 |
| 3494 | 1 | PETROLEUM SOUR CRUDE OIL, FLAMMABLE, TOXIC | I | Delete special provision 649 in column (6) of Table A. | This special provision was included in the consolidated versions of ADN 2011 when  UN No. 3494 was added on  1 January 2011, but it does not appear in document ECE/ADN/9 or subsequent documents containing the amendments to ADN 2009. Special Provision 649 was deleted from Chapter 3.3 as of 1 January 2011. | |
| 3494 | 2 | PETROLEUM SOUR CRUDE OIL, FLAMMABLE, TOXIC | II |
| 3494 | 3 | PETROLEUM SOUR CRUDE OIL, FLAMMABLE, TOXIC | III |
| 3537 | 1 | ARTICLES CONTAINING FLAMMABLE GAS, N.O.S. |  | Add special provision 802 in column (6) of Table A. | In ADR/RID, column (18) of Table A shows the corresponding special provision CV28/CW28 | |
| 3539 | 1 | ARTICLES CONTAINING TOXIC GAS, N.O.S. |  |
| 3540 | 1 | ARTICLES CONTAINING FLAMMABLE GAS, N.O.S. |  |
| 3541 | 1 | ARTICLES CONTAINING FLAMMABLE SOLID, N.O.S. |  |
| 3542 | 1 | ARTICLES CONTAINING A SUBSTANCE LIABLE TO SPONTANEOUS COMBUSTION, N.O.S. |  |
| 3543 | 1 | ARTICLES CONTAINING A SUBSTANCE WHICH IN CONTACT WITH WATER EMITS FLAMMABLE GASES, N.O.S. |  |
| 3544 | 1 | ARTICLES CONTAINING OXIDIZING SUBSTANCE, N.O.S. |  |
| 3545 | 1 | ARTICLES CONTAINING ORGANIC PEROXIDE, N.O.S. |  |
| 3546 | 1 | ARTICLES CONTAINING TOXIC SUBSTANCE, N.O.S. |  |
| 3547 | 1 | ARTICLES CONTAINING CORROSIVE SUBSTANCE, N.O.S. |  |
| 3548 | 1 | ARTICLES CONTAINING MISCELLANEOUS DANGEROUS GOODS, N.O.S. |  |

Table C, Identification No. 9004

3. Correction in the English, French and Russian versions:

Table C, Identification No. 9004, column (5)

Insert “9+” before “S”.

**Justification:**

* This difference/error has existed since ADN 2009.
* In column 5, all other entries are preceded by a dangerous goods class number before “S” for Sinker or “F” for Floater.

7.1.5.4.2 and 7.2.5.4.2

4. Amendment to 7.2.5.4.2: replace “7.2.3.15” with “8.2.1.2”.

**Justification**:

* Since ADN 2009, 7.2.5.4.2 has referred to 7.2.3.15 in the English and French versions, while it refers to 8.2.1.2 in the German version.
* Since ADN 2011, 7.1.5.4.2 has referred to 8.2.1.2 in all languages.
* Since the amendment to 7.2.3.15 was made in ADN 2013, the reference to “responsible driver” has not been clear. In the opinion of the German delegation, the presence on board of an expert who is not a driver is sufficient.

1. \* Distributed in German by the Central Commission for the Navigation of the Rhine under the symbol CCNR-ZKR/ADN/WP.15/AC.2/2021/19. [↑](#footnote-ref-1)
2. \*\* In accordance with the programme of work of the Inland Transport Committee for 2021 as outlined in the proposed programme budget for 2021 (A/75/6 (Sect. 20), para. 20.51). [↑](#footnote-ref-2)