|  |  |
| --- | --- |
|  | E/ECE/324/Rev.1/Add.47/Rev.10/Amend.6−E/ECE/TRANS/505/Rev.1/Add.47/Rev.10/Amend.6 |
|  |  | 3 December 2021 |

 Agreement

 Concerning the Adoption of Harmonized Technical United Nations Regulations for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these United Nations Regulations[[1]](#footnote-2)\*

(Revision 3, including the amendments which entered into force on 14 September 2017)

\_\_\_\_\_\_\_\_\_

 Addendum 47 – UN Regulation No. 48

 Revision 10 - Amendment 6

Supplement 19 to the 04 series of amendments – Date of entry into force: 30 September 2021

 Uniform provisions concerning the approval of vehicles with regard to the installation of lighting and light-signalling devices

This document is meant purely as documentation tool. The authentic and legal binding text is: ECE/TRANS/WP.29/2021/28.

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Paragraph 6.2.4.2.*, amend to read:

"6.2.4.2. In height: not less than 500 mm and not more than 1,200 mm above the ground. For category N2G, N3G, M2G, M3G (off-road) vehicles10 the maximum height may be increased to 1,500 mm."

*Paragraph 6.4.4.2.,* amend to read:

"6.4.4.2. In height: not less than 250 mm and not more than 1,200 mm above the ground. For category N2G, N3G, M2G, M3G (off-road) vehicles the maximum height may be increased to 1,400 mm."

*Paragraph 6.11.4.2.,* amend to read:

"6.11.4.2. In height: not less than 250 mm nor more than 1,000 mm above the ground. For rear fog lamps grouped with any rear lamp the maximum height may be increased to 1,200 mm. For categories N2G, N3G, M2G, M3G (off-road) vehicles the maximum height may be increased to 1,400 mm."

1. \* Former titles of the Agreement:

 Agreement concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958 (original version);

 Agreement concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions, done at Geneva on 5 October 1995 (Revision 2). [↑](#footnote-ref-2)