|  |  |  |
| --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2022/22 |
| _unlogo | **Economic and Social Council** | Distr.: General22 December 2021Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**186th session**

Geneva, 8-11 March 2022

Item 4.8.2 of the provisional agenda

**1958 Agreement:
Consideration of draft amendments to existing
UN Regulations submitted by GRSG**

 Proposal for Supplement 4 to the 01 series of amendments of UN Regulation No. 121 (Identification of Controls, Tell-tales, and indicators)

 Submitted by the Working Party on General Safety Provisions [[1]](#footnote-2)\*

The text reproduced below was adopted by the Working Party on General Safety Provisions (GRSG) at its 122nd session (ECE/TRANS/WP.29/GRSG/101, para. 90). It is based on ECE/TRANS/WP.29/GRSG/2021/30. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee (AC.1) for consideration at their March 2022 sessions.

*Table 1*, amend to read (revised footnote 16):
*"*

| *No.* | *Column 1* | *Column 2* | *Column 3* | *Column 4* | *Column 5* |
| --- | --- | --- | --- | --- | --- |
|  | *Item* | *Symbol* ***2*** | *Function* | *Illumination* | *Colour* |
| 42a. | Low tyre pressure(including malfunction) | Icon  Description automatically generated16 | Tell-tale | Yes | Yellow |
| 42b. | Low tyre pressure(including malfunction)that identifies affected tyre | VehicleDisplay_neg16, 17 | Tell-tale | Yes | Yellow |

…

16 Additionally, either of the low tyre pressure tell-tales may be used to indicate a tyre pressure monitoring system (TPMS), tyre pressure refill system (TPRS) and central tyre inflation system (CTIS) malfunction.

…"

1. \* In accordance with the programme of work of the Inland Transport Committee for 2022 as outlined in proposed programme budget for 2022 (A/76/6 (part V sect. 20) para 20.76), the World Forum will develop, harmonize and update UN Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)