**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**111th session**

Geneva, 9 - 13 May 2022 5 May 2022

Item 4 of the provisional agenda

**Work of the RID/ADR/ADN Joint Meeting**

Item 5 (b) of the provisional agenda

**Proposals for amendments to annexes A and B of ADR:**

**miscellaneous proposals**

 **Corrections to the draft amendments to ADR for entry into force on 1 January 2023 (ECE/TRANS/WP.15/256)**

 Revision

 **Note by the secretariat**

The secretariat reproduces hereafter proposals of corrections to the amendments to ADR for entry into force on 1 January 2023 as adopted by the Joint Meeting at its March 2022 session (Draft report: ECE/TRANS/WP.15/AC.1/2022/R.2/Add.4 / Final report: ECE/TRANS/WP.15/AC.1/164) and other editorial corrections.

 A. Corrections to ECE/TRANS/WP.15/256 adopted by the Joint Meeting

 *(ECE/TRANS/WP.15/AC.1/164)*

 Chapter 1.8, amendment to 1.8.6, 1.8.6.3.1 (f)

*For* quality management system *read* quality system

 Chapter 1.8, amendment to 1.8.7, 1.8.7.2.2.1 (f)

For the existing text, *substitute*

(f) The data contained in the documents for the type-examination according to 1.8.7.8.1, necessary for the identification of the type and variation, as defined by the relevant standards. The documents, or a list identifying the documents, containing the data shall be included or annexed to the certificate;

 Chapter 1.8, amendment to 1.8.7, 1.8.7.2.2.1

*Delete* the last sentence.

 Chapter 6.8, amendment to 6.8.2.1.23

For the existing text, *substitute*

6.8.2.1.23 Delete the last sentence of the first paragraph and corresponding footnote 7.

After the paragraph for “λ = 1”, insert the following new paragraph:

“The non-destructive checks of the circumferential, longitudinal and radial welds shall be carried out by radiography or by ultrasound. Other welds allowed in the appropriate design and construction standard shall be tested using alternative methods in accordance with the relevant standard(s) referenced in 6.8.2.6.2. The checks shall confirm that the quality of the welding is appropriate to the stresses.”

 Insert the following new paragraph immediately before the last paragraph:

 “Welds made during repairs or alterations shall be assessed as above and in accordance with the non-destructive tests specified in the relevant standard(s) referenced in 6.8.2.6.2.”

 Chapter 6.8, amendment to 6.8.2.2.2

For the existing text, *substitute*

6.8.2.2.2 Renumber current footnote 8 as footnote 7. At the end of the seventh paragraph, after “clearly apparent” insert a reference 8 to the following new footnote:

“**8***The mode of operation of dry break couplings is self-closing. Consequently, an open/closed indicator is not necessary. This type of closure shall only be used as a second or third closure.*”

 In the last sentence, delete: “or by a body designated by that authority”.

 Chapter 6.8, amendment to 6.8.2.4.1, 6.8.2.4.2 and 6.8.3.4.13

For the existing text, *substitute*

6.8.2.4.1, 6.8.2.4.2 and 6.8.3.4.13

 Amend footnote 12 to read:

“**12** In special cases, if agreed by the competent authority, the hydraulic pressure test may be replaced by a pressure test using gas, or if agreed by the inspection body, by using another liquid, where such an operation does not present any danger.”

 Chapter 6.8, amendment to 6.8.3.5.2, 6.8.3.5.3, 6.8.3.5.6, 6.8.3.5.11 and 6.8.3.5.12

*For* footnote 19(current footnote 18) *read* footnote 18

 Chapter 6.13 (previously 6.9), 6.13.1.1

*For* quality assurance programme *read* quality system

 Chapter 6.13 (previously 6.9), 6.13.4.4.2

*For* quality assurance programme *read* quality system

 B. Other corrections to ECE/TRANS/WP.15/256

 Chapter 1.6, amendment to 1.6.3.100.2

For the existing text, *substitute*

1.6.3.100.2 Replace “as from 1 January 2021” by “from 1 January 2021 to 31 December 2022 or 6.13.6.1 applicable as from 1 January 2023”.

 Chapter 4.1, amendment to 4.1.6.15, first paragraph

*For* Table 1 *read* Table 4.1.6.15.1

 Chapter 4.1, amendment to 4.1.6.15, table 4.1.6.15.1, for 4.1.6.8, fifth line, twice

Not applicable to English.

 Chapter 6.2, amendments to 6.2.2.3, sixth paragraph

Not applicable to English.

 Chapter 6.2, amendment to 6.2.2.11 renumbered as 6.2.2.12, in the table, third row under the heading row

Not applicable to English.

 Chapter 6.2, amendment to 6.2.2.11 renumbered as 6.2.2.12, second paragraph after the table

Not applicable to English.

 Chapter 6.2, amendment to 6.2.3.6.1, in the table, third row under the heading row

Not applicable to English.

 Chapter 6.2, amendment to 6.2.3.6.1, second paragraph after the table

*Insert* a paragraph break before the sentence starting with “Xa means”.

 Chapter 6.7, amendment to Note 1

Not applicable to English.

 Chapter 6.9, 6.9.1.1, second sentence

Not applicable to English.

 Chapter 6.13 (previously 6.9), 6.13.2.6

*For* ISO 527-2:2012 *read* EN ISO 527-2:2012

 Chapter 6.13 (previously 6.9), 6.13.4.2.2 (h) (ii), second indent

*For* (Tg) *read* Tg

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_