|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  | CorrigendumRef. Sales No. E.20.VII.3(ECE/TRANS/301, Vol. I and II)June 2022New York and Geneva |

**European Agreement concerning the**

**International Carriage of Dangerous Goods by**

**Inland Waterways (ADN)**

**(applicable as from 1 January 2021)**

 Corrigendum

|  |
| --- |
| *Note: As soon as they are issued, corrigenda to the published versions of ADN, as well as amendments entering into force before the next version, are made available on the United Nations Economic Commission for Europe web site at the following address: https://unece.org/transport/dangerous-goods* |

 1. Chapter 2.5, 2.2.52.4, entry for “ISOPROPYL sec-BUTYL PEROXYDICARBONATE+DI-sec-BUTYL PEROXYDICARBONATE+DI-ISOPROPYL PEROXYDICARBONATE”, column “Concentration”

For ≤ 32 + ≤ 15 – 18 ≤ 12 – 15 read ≤ 32 + ≤ 15 – 18 + ≤ 12 – 15

 2. Chapter 3.2, Table C, UN No. 1202, second entry, column (2)

*For* GAS OIL complying with standard EN 590:2013 + A1:2017 or DIESEL FUEL or HEATING OIL

*Read* DIESEL FUEL complying with standard EN 590:2013 + A1:2017 or GAS OIL or HEATING OIL

 3. Chapter 3.2, Table C, UN No. 3295 - HYDROCARBONS, LIQUID, N.O.S. CONTAINING ISOPRENE AND PENTADIENE, STABILIZED, 2 entries, column (5)

*For 3+inst. read 3+unst.*

 4. Chapter 3.2, 3.2.3.3, Scheme B, Columns 2, 3, 4, 5 and 6

*For* P d 50 *read* Pv50

 5. Chapter 7.2, 7.2.3.29.1, first indent

*For* Outboard motors *read* Petrol operated outboard motors

 6. Chapter 8.2, 8.2.2.4, heading

*For* Planning of refresher and specialization courses r*ead* Planning of basic and specialization courses

 7. Chapter 9.3, 9.3.1.14.2, 9.3.2.14.2 and 9.3.3.14.2, subparagraph (a)

*For* non-watertight *read* non-weathertight

 8. Chapter 9.3, 9.3.1.14.2, 9.3.2.14.2 and 9.3.3.14.2, subparagraph (b)

*For* non-watertight *read* non-weathertight

 9. Chapter 9.3, 9.3.1.15.2, last sentence of last paragraph

*For* non-watertight *read* non-weathertight

 10. Chapter 9.3, 9.3.2.15.2, last sentence of last paragraph

*For* non-watertight *read* non-weathertight

 11. Chapter 9.3, 9.3.3.15.2, last sentence of last paragraph

*For* non-watertight *read* non-weathertight