|  |  |  |
| --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.15/AC.1/2023/2 |
| _unlogo | **Economic and Social Council** | Distr.: General21 November 2022Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**Joint Meeting of the RID Committee of Experts and the
Working Party on the Transport of Dangerous Goods**

Bern, 20-24 March 2023

Item 5 (b) of the provisional agenda

**Proposals for amendments to RID/ADR/ADN:
new proposals**

 RID/ADR Table A: UN 3550, missing code for mixed packing in column (9b)

 Transmitted by the Government of Germany[[1]](#footnote-2), [[2]](#footnote-3)\*\*

 Introduction

1. Germany has noted that in the amendment instructions for RID/ADR applicable from 1 January 2023 for the new entry:

UN 3550 COBALT DIHYDROXIDE POWDER, containing not less than 10% respirable particles,

it was forgotten to add the code for mixed packing in column (9b) of Chapter 3.2, Table A.

2. For entries in Table A where there is no code in column (9b), only the general requirements apply in accordance with the explanatory notes in RID/ADR 3.2.1 concerning column (9b) (see 4.1.1.5 and 4.1.1.6).

3. For all other entries of Class 6.1, classification code T5, packing group I, the code “MP18” is shown in Table A, column (9b):

“May – in quantities not exceeding 0.5 kg per inner packaging and 1 kg per package – be packed together in a combination packaging conforming to 6.1.4.21:

– with goods of other classes, except Class 7, when mixed packing is also permitted for these; or

– with goods which are not subject to the requirements of RID/ADR,

provided they do not react dangerously with one another.”

4. Germany recommends that code “MP18” should also be shown for UN number 3550.

 Proposal

5. In RID/ADR Table A, Chapter 3.2, Germany proposes to insert code “MP18” in column (9b) for the new UN number 3550.

1. A/77/6 (Sect. 20), table 20.6 [↑](#footnote-ref-2)
2. \*\* Circulated by the Intergovernmental Organisation for International Carriage by Rail (OTIF) under the symbol OTIF/RID/RC/2023/2. [↑](#footnote-ref-3)